Test request form

AGGREGATES FOR SEALING WORKS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| TO: | PANEL CONTRACTOR | | Contact: | | **Panel contractor contact number** |
| CC | DPI CLERK | | Test Request Number: | | **Ascending number reference** |
|  | |  | |  | |
| PROJECT: | | NAME OF PROJECT – AS PER SPEC | | PAGE 1 OF 1 | |

* When required, in accordance with the contract documents, order the conformance testing in WRITING DIRECTLY from the Panel Period Contractors.
* Should the next Panel Period Contractor on the list *not* be available to perform the required testing, notify the Superintendent immediately.
* Give the Panel Period Contractor written notice in advance of each stage of the works requiring conformance testing, including re-testing.
* Notice – Provide the Superintendent with a copy of the order for testing simultaneously with the order being sent to the Panel Period Contractor.
* Any communication with the Panel Period Contractors, other than the ordering of testing or inquiring on the timing of test results must be forwarded through the Superintendent.
* Provide the Superintendent with the results of process control testing as identified in the relevant ITP with all requests for conformance testing.
* Notice – Notify the Superintendent prior to any rework of failed lots.

DATE & Time test REQUIRED: REASONABLE notice required to be given to panel PERIOD CONTRACTORS – ENSURE TIMES FOR TESTING REFLECT THE ACTUAL PROPOSED COMPLETION TIME OF THE LOT TO BE TESTED.

Lot Number: clearly identify number of THE LOT – EASIER FOR EVERYONE

Start chainage: ENSURE THIS IS Clearly marked on site – related to lot numbers

Finish chainage: ENSURE THIS IS clearly marked on site – related to lot numbers

Width (m): width of ROAD OR AREA to be tested

Length (m): length of the lot – TAKEN FROM CHAINAGES

Test & Layer depth: n/A

layer type: n/a

Tests REQUIRED: TESTING IS TAKE PLACE ON SITE – WHAT MATERIALS ARE TO BE USED FOR SEALING - NO QUARRY RESULTS ARE TO BE ACCEPTED

MINIMUM 3 SAMPLE TO BE TESTED ONCE YOU GET ABOVE 750 TONNE THEN 1 EXTRA TEST PER EVERY 250 TONNE TO BE USED (IE 1200 TONNE - 5 SETS OF TESTS REQUIRED)

PSD – (MINIMUM 3)

ALD – (MINIMUM 3)

FI – (MINIMUM 3)

CONTRACTOR: CONTRACTORS NAME CONTACT NO: CONTRACTORS PHONE No

DATE & TIME: SENT FAX NO: AS ABOVE